{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Hardware Update Record"],"not_rendered":{"external_links":2,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Hardware Update Record","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"merged":[[1,0,1,7],[2,0,3,7],[5,0,6,0],[7,0,8,0],[9,0,10,0],[11,0,12,7],[14,0,19,0],[20,0,21,0],[22,0,23,0],[24,0,25,7],[27,0,28,0],[29,0,30,0],[31,0,35,0],[36,0,39,0]],"flags":["formulas_cached_only"]}
[]
["7206V10B_RB_A Hardware Version Update Record"]
["7206V10B_RB_A Ver.A"]
[]
["Change item","NO.","Change Description"," Description","Page","priority","Modified Date","Modified by"]
["SCH",null,null,"The 1st release Version"]
[]
["PCB",null,null,"The 1st release Version"]
[]
["BOM",null,null,"The 1st release Version"]
[]
["7206V10B_RB_A Ver.B"]
[]
["Change item","NO.","Change Description"," Description","Page","priority","Modified Date","Modified by"]
["SCH",1,"Add R337","Solve the problem of configuration errors when powering on with an SD card","P11","important",6.24,"XT"]
[null,2,"Update U10","Update the package of SOC for easier soldering","P6/7","optional",6.24,"XT"]
[null,3,"Replace L2 and C21","Optimize the parameters of SM8002","P5","important",8.25,"XT"]
[null,4,"Replace U16","To reduce ripple noise","P6","important",8.25,"XT"]
[null,5,"Delete R104","Prevent the power supply of the serial port board from flowing back from R104 to the DEMO board","P9","important",8.25,"XT"]
[null,6,"Delete C102 and Replace R108,R337","Solve the problem of configuration errors when powering on with an SD card","P11","important",8.25,"XT"]
["PCB",1,"Follow SCH"]
[]
["BOM",1,"Follow SCH"]